## RELAYER commands

## RELAYER specific commands

GMAC get mac address

Response: MAC=xx:xx:xx:xx:xx:xx (the mac address for this node)

SYSI get All Node and Device Info from all nodes.)

This is done by issuing a 'GNOI' and 'GDEI' command to all known

nodes (see GNDI and GDEI below for each node's repsonse);

GVER Get the version of a specific device.

## NODE specific commands

SNNA|<name> Set the node name

GNOI get Node info

GDEI get Device Info

PING <respond to relayer with PONG>

BLIN Blink the LED 10 times

RSET Reset

## DEVICE specific commands

// GDNA Get device name

// SDNA Set device name

// ENIP Enable immediate processing

// DIPP Disable immediate processing

// DOIP Do immediate one time processing

// ENPP Enalble periodic processing

// DIPP Disable periodic processing

// DOPP DO periodic processing (one time)

// GRAT Get periodic processing rate ( calls per hour)

// SRAT Set periodic processing rate ( calls per hour)

// GDVR Get Version (of driver)